

WIDTH ADJUSTER CH1

WIDTH ADJUSTER CH0

100 kHz

EXT TRG

TO DIGITIZER TRG IN

TO LASER TRG IN

Converter

NIM TTL